African Endurance Racing – Appendix A Fuel Rig Regulations.
A. FIA approved single and twin fuel nozzle systems.
The refuel systems must carry a current FIA label of approval as per appendix 252-7 of the FIA Regulations which is available on the FIA website as a down load.

B. Non FIA Fuel Rigs with a standalone Fuel Tank.
1. Only a single refueling hose system may be used.

2. The fuel dispenser hose must be fitted with a shutoff nozzle at its exit to the car fuel tank.

3. The hosing used must be to S.A.B.S standards.

4. The fuel rig tank maximum capacity is 200L.

5. The top of the fuel rig tank may not be higher than 2000mm from the rig base ground level.

6. The maximum external diameter of the fuel rig tank may not exceed 1000mm.

7. The minimum diameter of the fuel rig base may not be less than 1500mm.

8. The fuel rig tank must be fitted with a vent pipe on top of the rig fuel tank and the vent pipe shall have a flame trap fitted to its outer end. The vent pipe shall be of a minimum of 13mm internal diameter and a minimum length to 1000mm from fuel tank top to flame trap base.

9. A Manual shut off valve will be fitted between the fuel tank and the outlet hose directly at the tank end.

10. The fuel rig must be earthed to ground via a minimum 10mm earth cable.

11. The car being refueled must be earthed via a detachable cable.
C. FIA approved Fuel Churns.
1. FIA approved Fuel churns as supplied by race parts suppliers and as used by various FIA series may be used. The churns must be of the type equipped with an anti blow back system.
D. Non FIA approved Fuel Churns.
1. Non FIA approved fuel churns may be used as long as they meet the requirements of  the event scrutineers as  follows:

2. The churn may not hold more the 30l.

3. The churn outlet nozzle must be a minimum length of 150mm.

4. The vehicle being refueled must be fitted with a second fuel tank outlet pipe to which must be attached a clear detachable overflow tank with a minimum capacity of 20l. There must be a leak proof connection between the car tank and the clear overflow tank to avoid spillage.

E. 1. No Other systems are allowed.

