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The African 6 Hour 2014

22rd February 2014 (Provisional)


In addition to the Supplementary Regulations issued for the event, these basic rules and regulations will apply as if they form part of said Supplementary Regulations:

A. General.

1. The African 6 Hour is open by invitation to all Saloons and Sports & GT closed wheel cars complying with 2013/14 technical regulations as published by MSA or the FIA in the case of LMP1 & LMP2 cars and GTE-Pro and GTE-Am.

2. No “special” vehicles which are not part of a recognised 2014 MSA or FIA category will be allowed to compete. It is the responsibility of the entrant to prove eligibility.

B. Entries.

1. The entry fee for the event is R3500.00 which includes MSA fees, transponder fees for one car and three drivers. 12 team tickets will be issued per team. 

2. Entries open immediately and close on the 31St December 2013. Entries must be sent to:

Classic Car Events

Po Box 590

Pinegowrie 2123

roger@afriod.co.za
+27117897135 fax

C. Teams and Drivers.

1. No relay teams are permitted.

2. A maximum of three drivers per car is allowed and no driver may drive for more than two hours continuously with a minimum break of 15 minutes between the two hour periods.

3. Drivers may only drive for one entry.

4. Each Team must have a Team Manager who may not be a driver or technician.

D. Tyres.

1. Tyre type and size is free.

E. Classes.

1. Classes are based on capacity.

2. Saloon Cars:


Class E
up to 1299cm


Class F

1300cm to 1599cm


Class G
1600cm to 1999cm


Class H
2000cm to 2999cm


Class I

3000cm to 4999cm


Class J

over 4999cm

3. Sports Racing Cars:

Class A LMP1

Class B LMP2

Class N over 4999cm

Class P 3000cm to 4999cm

Class R 2000cm to 2999cm

Class S 1300cm to 1999cm

Class T up to 1299cm

A 5% oversize in capacity will be allowed in each class.

4. Production Sports & GT Cars:

Class C GTE-Pro

Class D GTE-Am

Class U over 4999cm

Class V 3000cm to 4999cm

Class W 2000cm to 2999cm

Class X1600cm to 1999cm

Class Y 1300 cm to 1599cm

Class Z up to 1299cm

A 5% oversize in capacity will be allowed in each class.

5. Capacity for classing where required will be taken as the ACTUAL declared capacity of the competing vehicle less the 5% allowance. 

6. The penalty for false declaration will be exclusion from the event.

7. Cars with forced induction and all Rotary engined cars will be subject to an equivalency factor of 1.4 by which their actual capacity will be multiplied to determine a capacity for classing purposes. 

8. Forced induction Rotary engines will be subject to an equivalency factor of 2.0

F. Scoring.

1. All drivers competing in the six hour Endurance Race will be eligible to compete for:

2. Overall 1st to 3rd.

3. Class from 1st to 3rd place if sufficient entries per class.

4. Index of Performance 1st. 
5. The Index of Performance will be scored as a separate competition.

G. Trophies.

1. Overall:

1st overall 

2nd overall

3rd overall

2. Index:

1st overall

3. Class:

1st to 3rd depending on entries

H. Qualification as a finisher.  

1. A competing car must cross the finishing line on the circuit, after the chequered flag has been shown, to qualify as a finisher. 

2. The competing car must have completed 66% of the race distance to qualify as a finisher. 

3. Race distance will be defined as the number of laps completed by the fastest car in each class. Should there be only one car in a class the organisers will determine a race distance.

4. The pit lane exit will be closed 5 minutes before the the chequered flag is shown.

5. Only cars that have completed the race and have been classified as a finisher may score towards Index of Performance.

I. In car timing.

1. In car timing is permitted. 

J.  In car communications.

1. In car communication (ship to shore) is recommended. 

K. Qualifying.

1. Qualification times will only be taken from the official qualifying session for the event. 

2. Drivers failing to qualify in the session will be placed at the back of the grid. 

3. Only one driver need qualify but all drivers must participate in the night timed practice between 7.00pm and 8.00pm on Friday the 21st February 2014.

4.  A minimum qualifying time may be applied and only 60 cars will be allowed to start. 

L. Safety Car Period

1. During the Endurance race, pitting for driver change or refuelling is allowed during safety car periods.

M.  60KpH Board.

1. A 60 board may be shown which means that all cars shall drop to an estimated speed of 60kph and shall hold position until a green flag replaces the 60kph board.

2.  No overtaking is allowed during a 60kph period.

3. This board will be used to assist the recovery of vehicles should they fail during the event and need to be returned to the pits for repair so as to continue the event.

N.  Fuel.

1. A maximum fuel tank capacity of 100L is allowed. Petrol and Diesel Fuels are allowed. 

2. Methanol based fuels are not permitted.

O. Refuelling.

1. Only refuelling equipment described in Appendix “A” of these regulations may be used.

2. A maximum of 3 crew members may refuel the car whilst the car is on Pit Road at all times before or during the event.

3. Drivers may not be in a car during refuelling and may not enter a car until the refuel operation is complete and he/she is advised by the Team Manager that it is safe to enter the car.

4. The car engine must be shut down during refuelling and may not be started until refuelling is complete and advised safe to do so by the Team Manager.

5. One person shall man the fuel nozzle into the car, another shall hold a 9kg at the ready and another shall man a manual fuel shut off valve at the base of the refuelling rig.

6. The three refuelling persons shall be attired with a fire proof balaclava, fire proof gloves and protective cotton clothing covering the arms and legs. 

7. A cotton boiler suit is ideal. Nylon, Plastic or synthetic derivative clothing of any sort is not allowed.

8. An incoming or outgoing suitably attired driver may take any of the three refuelling positions but not in addition to.

9. The Team Manager may advise but may not take part in any refuelling operation.

10. Car fuel tanks must be equipped with suitable ventilation to avoid blow back whilst refuelling

.

11. Refuelling from cans, drums etc are not permitted. Only equipment described in Appendix A may be used.

12. No refuelling is allowed in the Pit Garage.

13. No manual, electric, hydraulic pumps or pressure devices are allowed to refuel a car. Cars must be refuelled by gravity feed.

14. Bulk fuel must be stored behind the Pit Garage and may not be in the Pit Garage or Pit Front at any time except to refuel the fuel rig.

15. Bulk fuel containers may not be in the Pit Garage of the Pit Front during the race.

16. The refuelling of fuel rigs with electric pumps is not permitted. Only manual pumps may be used.

Fuel spillage during a refuel will result in a one lap drive through penalty.

Contravention of any of items 1 to 16 above will result in exclusion from the event.

P.  Pit Lane.

1. Only three technicians are allowed to work on a car whilst it is stopped in front of the Pit Garage on Pit Lane.

2. The Team Manager may only advise on the Pit Lane.

3. Drivers may be part of the three technicians but not in addition to.

4. No work is allowed on the car whilst it is being refuelled.

5. Wheels may be changed on the Pit Lane.

6. Lubricants may be checked and topped up on the Pit Lane.

7. Cars or parts thereof may be cleaned on the Pit lane.

8. Drivers may be assisted to enter or exit a car on Pit lane but not during a refuel.

9. Cars may not be push started during the race and the penalty for doing so is a drive through penalty.

10. A maximum speed of 60kph in Pit Lane is allowed at any time. The penalty for exceeding the 60Kph limit is a drive through penalty.

11. Any other work than that described above must be performed in the Pit Garage.

12. No smoking is permitted between the 5 metre drain line behind the Pits and the Pit wall.

13. A maximum of SIX people are allowed on the Pit Lane at any time.

14. The PIT LANE is designated as the concrete area in front of each Pit Garage as 

              Per APPENDIX “B”      
Q. Pit Garage.

1. Car engines may not be stated in the Pit Garage.

2. Cars must be pushed into and out of a Pit Garage.

3. There is no restriction on how many people may work on a car in a Pit Garage.

4. No fuel may be stored in the Pit Garage.

5. No smoking, alcohol or children under the age of 16 (sixteen) are permitted in the Pit Garage at any time.

6. No repairs may be undertaken outside of the Pit Garage.

7. If any major components are changed during the race approval must be obtained from the Chief Scrutineer to rejoin the race.

8. The rear of the Pit Garage must be kept clear of any vehicles at any time. The rear of the Pit Garage extends to the concrete drain as per Appendix “C”.

R. Pit Wall.

1. Only three people from a team are allowed on the Pit Wall during the race and practices.

2. Each Team will be issued with 2 (Two) Pit Lane lanyards and 1 (One) Team Manager Lanyard and only persons carrying these lanyards will be allowed onto the pit wall.

3. The Pit Lane exit will close 5 (Five) minutes before the finish flag is displayed. Once the Pit Lane exit is closed items 17.1 and 17.2 will be derestricted.

S. Formation Laps 

1. 15 Minutes Prior to the start of the race, the pit lane will be opened.

2. Competitors may complete an installation lap and form up on the grid in starting order. 

3. Should an additional installation lap be required, the competitor may do so by driving down the pit lane.

4. The pit lane will be closed 5 minutes before the scheduled start time. 

T. Outside assistance.

1. In the event of a car breaking down on the circuit, no outside assistance is permitted other than by the track marshals moving the car to a safe position if it is deemed to be unsafe. Such assistance may not be used to restart the engine.

2. Only the driver is permitted to make repairs and only with tools carried on the vehicle. 

3. No refuelling or replenishment of oil or water is allowed on circuit other than in the designated pit area. 

4. No additional fuel may be carried in the vehicle other than in the designated fuel tank.

5. No other person except the track marshals or driver may touch the car outside of the pit area or starting grid.

6. The organisers will make every effort to return the car to the pits for repair. (See 60Kph board) and a recovery vehicle will be sent to collect a car, under caution, if required.

U. Lights.

1. All vehicles competing in the African 6 hour will be required to have the following operating at scrutineering:

2 x Operating Headlamps
            1 x Operating Tail Lamp

1 x Operating Brake Light if required under category regulations.

4 x working indicators where originally fitted to the vehicle and as per category regulations.

2. A maximum of two additional front facing spotlights may be fitted.

3. A maximum of two forward or left hand side facing marker or lights may be fitted in a non white colour.

4. Light must be turned on at 6.30pm during the race.

5. A car will be given two laps to comply with U.4 where after it will be called into the pits for repair or to comply.

6. Should weather conditions require a different (ie brought forward) “lighting up” time, and at the Clerk of the Course’s discretion, a LIGHT ON board will displayed at the start line for 3 Laps. 

7. Non compliant vehicles will be black flagged and must return to the pits for repairs to the lights and inspected by an official of the meeting for compliance before returning to the circuit.

V. Communications and Timing.

1. The event will operate as a wireless (Wi-Fi) system and there will be no paper records.

2. An additional server and three boosters will be fitted to the Pit Garages.

3. Teams must be equipped with the necessary Lap Tops, Pcs etc to follow the progress of the event and to receive instructions.

4. The Pit Lane Director will back up and enforce any instructions received from the C.o.C.

5. The Pit Lane Director will ONLY communicate with the Team Manager.

6. Any queries on the technical requirements must be directed to Andre Furby at andre@protiming.co.za
7. Each driver shall have a separate timing transponder which must be changed at every driver change during practice sessions and the race.

W. Car Recognition.

1. Every effort will be made to use the race number as requested on the entry form and these numbers will be recognised on a first come first served basis.

2. It will be the responsibility of the Team to make sure that the car is fitted with the correct number as advised by the organisers where a number change is required.

3. It is compulsory to fit to the car decals showing the drivers name, Country of Domicile and Blood Group.

4. The organisers reserve the right to fit sponsors decals to a car.

X. Documentation & Scrutineering.

1. Documentation will take place on Friday the 21st between 9.00am and 12.00pm.

2. Scrutineering will take place between 9.00am and 4.00pm on Friday the 21st.

Y. Camping.

Camping is permitted behind the Cafeteria area.

Z.  Trailer Park.

Trailer must be parked in the designated area to the right of the Cafeteria.

African Six Hour Appendix “A”

A. Fuel Rigs fitted with quick Fit Nozzles.

1. The nozzle type fuel rig must comply with FIA Specification J252-7. There are no exceptions to this rule.

2. Single nozzle quick fit fuel fillers are NOT permitted.

B. Fuel Rigs with Single Nozzle manually operated.

1. The maximum capacity of the fuel rig tank is 200L.

2. The maximum diameter of the fuel rig tank is 900mm.

3. The base of the fuel rig stand must be a minimum of 1000mm diameter.

4. The maximum height from the ground to the base of the fuel rig tank is 2000mm.

5. A 13mm I.D. vent pipe must be fitted to the top of the fuel rig tank and the length of the pipe is 1000mm. A flame trap should be fitted to the pipe outlet.

6. A shut off valve must be fitted between the fuel rig tank and the fuel delivery hose.

7. The fuel delivery hose must be to garage forecourt specifications.

8. An automatic blow back cut-off type hand operated fuel dispensing nozzle, as used on garage forecourts, must be fitted to the delivery end of the hose.

9. The fuel rig must be earthed to ground before use.

C. Refuelling by means of drums, cans and siphon hoses.

1.  Refuelling by the above methods is not permitted.

2. Only FIA approved fuel churns may be used for this method of refuelling.

Note. All cars must be connected to an earth or anti static cable whilst refuelling.

African Six Hour 2014 “Appendix B”

1. The concrete area in front of the pits is the designated “PIT LANE”

2. The tar area in front of the pits is “PIT ROAD”

3. The blue wall opposite the pits is the “Pit Wall”
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